Everyone will begin as a Tier One (Green Level) and everyone will get 1 FREEBIE RUN (No extra equipment needed) Tier One Level 4wheelers can choose from any of the runs designated this level.  After your FREEBIE RUN in order to do another trail you will need the following equipment: 

• A working CB Radio that works well on trail – hand held’s are questionable -  it’s important for the entire group to be able to hear you. 

• A current year OHV sticker – support Colorado & the trails we love. 

• Fire extinguisher. 

First aid kit – band aids / pain meds / Tylenol / aspirin/ 

• If you are planning on airing down before the run, you must have an air compressor or air tank of some sort.   To advance to Tier Two status, you must attend at least 2 Tier One events. You must schedule a time to meet with a leader and show your required equipment and your knowledge of  equipment and ability. If scheduled in advance this can be done during or after a tier one event.
To attend Tier Two level runs: 

• You must be comfortable with Tier One runs 

• You will have the ability to tackle moderate obstacles without a spotter. If a spotter is needed you will be able to take direction. 

• You will need a suspension lift and minimum 33” off-road tires. 

• Must show proof of equipment required suggesting:  (defined by RS members)


 Basic Tool kit, Spill Kit, Fluids (oil, anti-freeze, wd-40, starting fluid, brake fluid, atf, gear oil) ,   bottle jack & stackable blocks of wood, or hi-lift jack (knowledge to use)  D-rings, Tree hugger (no winch around a tree) , tow strap or Bubba rope, Snatch block. 

To advance to Tier Three status, you need to have a minimum of 5 runs with the group as well as attend and pass an on-trail winch test and obstacle test.

To attend Tier Three level runs:

 • You must complete Tier Two requirements and be comfortable with Tier One and Tier Two. 

• You must have knowledge of line choice and  be willing to assist.

• Must have all Tier 2 equipment PLUS:

 • A working winch 

• Minimum tire size of 35” 

• Locker (s) 

• Skid Plates. 

To advance to Tier Four status you must have a minimum of 10 runs

Tools • Screwdrivers Flat & Phillps • Metric Wrenches up to a 24mm • Sockets 3/8 Drive up to 36mm Sockets • Sockets SAE and/or Metric or Both • Extensions • Pliers • Channel Locks • Crescent Wrench • Vice Grips • Pry Bar Adjust. or Fixed Multiple Sizes • Torques Bits & Allen Wrenches • ½” Drive Breaker Bar • Zip Ties, Duct or Gorilla Tape • Jumper Cables or Jump Pack • Tire Repair Kit with valve cores • Bailing Wire & Nylon Rope • Spill Kit – Absorption Pad or liquid catch, Kitty Litter Electrical Tools & Fluids • Dikes & Strippers • Electrical Fittings (crimp or heat) • Electrical Tape • Fuses • Wire Crimpers • Wire 10-18 Gage – Sml. Rolls Fluids to Include: • 2 QRTS. Oil • 1 GAL. Anti-Freeze • WD 40 & Starter • Brake Fluid DOT 3 or Higher • 2 QRTS. ATF + 4 • 1 QRT. 85 140 Gear Fluid • JB Weld sml. tube or Red & Tacky Recovery Equipment • Bottle Jack and a block of wood or stackable blocks or Hi Lift Jack (knowledge of how to use) • D-Rings – Ones with a higher weight capability 7 in reach • Tree Hugger – you may NEVER wrap a winch line around a tree • Tow Strap and/or Bubba Rope (3) Same strength and len
